{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["IMPERIAL","METRIC"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"IMPERIAL","index":0,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["UNEVEN BOX JOINTS WITH UNIFORM SPACING"]
["WORK PIECE WIDTH CALCULATION"]
[]
["NORTH AMERICAN JIGS"]
["IMPERIAL DC MODELS"]
[]
[]
[]
[]
[]
["Important Notes:"]
[]
["Use the half blind pin guides and universal tail guides"]
["Use the .350\" Box Joint Cutter"]
["Use an AKEDA precision 7/16\" guide bushing."]
["          Its internal diameter (.385\") clears the .350\"  cutter"]
["Make sure the cutter is centered in the guide bushing and that they do not touch"]
["Start and end with a half \"pin\""]
["Don't rout on the outsides of the first and last pin guides"]
[]
[]
[]
["YOU CAN VARY THIS DATA",{"$nulls":5},"FIXED DATA",null,"THIS IS THE RESULTING DATA"]
[]
["Enter data in the green boxes:",{"$nulls":7},"Do not enter data in these boxes:"]
[]
["A",{"$nulls":5},"B",null,"C",null,"D",null,"E"]
[{"$nulls":8},"( A + B )"]
["ENTER THE",null,"HOW MANY",null,"HOW MANY",null,"FULL \"PINS\"",null,"THIS WILL",null,"THIS WILL",null,"THIS WILL",null,"THIS WILL"]
["DESIRED \"TAIL\"",null,"1/8\" INCREMENTS",null,"FULL \"PINS\"",null,"ARE ALWAYS",null,"BE THE",null,"BE THE",null,"BE YOUR",null,"BE THE"]
["SIZE IN",null,"PAST THE REF.",null,"DO YOU WANT?",null,"THIS SIZE",null,"GUIDE",null,"SIZE OF EACH",null,"WORK PIECE",null,"NUMBER"]
["INCREMENTS",null,"MARK IS THE FIRST",{"$nulls":5},"FINGER",null,"LH AND RH",null,"WIDTH",null,"OF \"TAILS\""]
["OF 1/8\"",null,"GUIDE FINGER?",{"$nulls":5},"PITCH",null,"HALF \"PIN\""]
[]
[]
[0.625,null,2,null,3,null,0.375,null,1,null,0.4375,null,4.5,null,4]
[]
["Enter a minimum of 0.625",null,"1 or 2 increments",null,"Related to your",null,"Do not change",null,"Minimum 1.0",null,"Compare to",null,null,null,"Always one more"]
["or choose from 0.75,",null,"look best (column \"D\"",null,"work piece width",null,"this number!",null,null,null,"size of full \"pin\"",null,null,null,"than the number"]
["0.875, 1.0, 1.125",null,"to see how it looks)",{"$nulls":11},"of full \"pins\""]
["and so on."]
[]
[]
["Note - Box joints can also be cut with variable spacing in 1/8\" increments!"]

{"sheet":"METRIC","index":1,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["UNEVEN BOX JOINTS WITH UNIFORM SPACING"]
["WORK PIECE WIDTH CALCULATION"]
[]
["JIGS OUTSIDE NORTH AMERICA"]
["METRIC DC MODELS"]
[]
[]
[]
[]
[]
["Important Notes:"]
[]
["Use the half blind pin guides and universal tail guides"]
["Use the 8.9 mm Box Joint Cutter"]
["Use an AKEDA precision 11.1 mm guide bushing"]
["          Its internal diameter  clears the 8.9 mm  cutter"]
["Make sure the cutter is centered in the guide bushing and that they do not touch"]
["Start and end with a half \"pin\""]
["Don't rout on the outsides of the first and last pin guides"]
[]
[]
[]
["YOU CAN VARY THIS DATA",{"$nulls":5},"FIXED DATA",null,"THIS IS THE RESULTING DATA"]
[]
["Enter data in the green boxes:",{"$nulls":7},"Do not enter data in these boxes:"]
[]
["A",{"$nulls":5},"B",null,"C",null,"D",null,"E"]
[{"$nulls":8},"( A + B )"]
["ENTER THE",null,"HOW MANY",null,"HOW MANY",null,"FULL \"PINS\"",null,"THIS WILL",null,"THIS WILL",null,"THIS WILL",null,"THIS WILL"]
["DESIRED \"TAIL\"",null,"1/8\" INCREMENTS",null,"FULL \"PINS\"",null,"ARE ALWAYS",null,"BE THE",null,"BE THE",null,"BE YOUR",null,"BE THE"]
["SIZE IN",null,"PAST THE REF.",null,"DO YOU WANT?",null,"THIS SIZE",null,"GUIDE",null,"SIZE OF EACH",null,"WORK PIECE",null,"NUMBER"]
["INCREMENTS",null,"MARK IS THE FIRST",{"$nulls":5},"FINGER",null,"LH AND RH",null,"WIDTH",null,"OF \"TAILS\""]
["OF 2.5 mm",null,"GUIDE FINGER?",{"$nulls":5},"PITCH",null,"HALF \"PIN\""]
[]
[]
[16,null,2,null,3,null,"9.0",null,25,null,9.75,null,110.5,null,4]
[]
["Enter a minimum of 16.0",null,"1 or 2 increments",null,"Related to your",null,"Do not change",null,"Minimum 25.0",null,"Compare to",null,null,null,"Always one more"]
["or choose from 18.5,",null,"look best",null,"work piece width",null,"this number!",null,null,null,"size of full \"pin\"",null,null,null,"than the number"]
["21.0, 23.5, 26.0",{"$nulls":13},"of full \"pins\""]
["and so on."]
[]
[]
["Note - Box joints can also be cut with variable spacing in 2.5 mm increments!"]